Chapter 7

Revision 1.66 Page 357

Graphics State Summary

The following tables summarize the variables that make up the Graphics State.

Nearlyallofthe Graphics State variables have a default value as shown below.

That value is reestablished for ev eryglyph in a font. Instructions are available for resetting the value ofallGraphics State variables. Some state variables can be reset in the CVT Program. In such cases the value set becomes the new default and willbe reestablished for each glyph. When value ofa state variable is changed byinstructions associated with a particular glyph, it willhold only for that glyph.

The setting ofthe Graphics State variables willaffect the actions ofcertain instructions. Affected instructions are listed for e ach variable.

Graphics State Variable Default Set With Affects auto_flip TRUE FLIPOFF

FLIPON

MIAP

MIRP control_value_cut_in 17/16 pixels SCVTCI MIAP

MIRP delta_base 9 SDB DELTAP1

DELTAP2

DELTAP3

DELTAC1

DELTAC2

DELTAC3 delta_shift 3 SDS DELTAP1

DELTAP2

DELTAP3

DELTAC1

DELTAC2

DELTAC3 dual_projection_vectors ˙ SDPVTL IP

GC

MD

MDRP

MIRP

Page 358 Revision 1.66

freedom_vector x - axis SFVTCA

SFVTL

SFTPV

SVTCA

SFVFS

GFV gep0 1 SCE0

SCES

AA

ALIGNPTS

ALIGNRP

DELTAP1

DELTAP2

DELTAP3

IP

ISECT

MD

MDAP

MIAP

MIRP

MSIRP

SHC

SHE

SHP

UTP gep1 1 SCE1

SCES

AA

ALIGNPTS

ALIGNRP

IP

MD

MDRP

MIRP

MSIRP

SHC

SHE

SHP

SFVTL

SPVTL

Revision 1.66 Page 359

gep2 1 SCE3

SCES

ISECT

IUP

GC

SHC

SHP

SFVTL

SHPIX

SPVTL

SC instruct_Control 0 INSTCTRL all instructions loop 1 SLOOP ALIGNRP

FLIPPT

IP

SHP

SHPIX minimum_distance 1 pixel LMD MDRP

MIRP projection_vector x - axis SPVTCA

SPVTL

SVTCA

SPVFS

GPV round_state 1 RDTG

ROFF

RTDG

RTG

RTHG

RUTG

SROUND

S45ROUND

MDAP

MIAP

MDRP

MIRP

ROUND rp0 0 SRP0 IP

MDAP

MIAP

MIRP

MSIRP

SHC

SHE

SHP

Page 360 Revision 1.66

rp1 0 SRP1 IP

MDAP

MDRP

MIAP

MSIRP

SHC

SHE

SHP r p2 0 SRP2 IP

MDRP

MIRP

MSIRP

SHC

SHE

SHP scan_control FALSE SCANCTRL

SCANTYPE singe_width_cut_in 0 pixels SSWCI MIAP

MIRP single_width_value 0 pixels SSW MIAP

MIRP